### Avoiding Trouble

Many procedures in this book require you to "label and disconnect . . . '' a group of lines, hoses or wires. Don't be lulled into thinking you can remember where everything goes — you won't. If you hook up vacuum or fuel lines incorrectly, the vehicle will run poorly, if at all. If you hook up electrical wiring incorrectly, you may instantly learn a very expensive lesson.

You don't need to know the official or engineering name for each hose or line. A piece of masking tape on the hose and a piece on its fitting will allow you to assign your own label such as the letter A or a short name. As long as you remember your own code, the lines can be reconnected by matching similar letters or names. Do remember that tape will dissolve in gasoline or other fluids; if a component is to be washed or cleaned, use another method of identification. A permanent felt-tipped marker can be very handy for marking metal parts. Remove any tape or paper labels after assembly.