### Engine Fan

#### REMOVAL & INSTALLATION

1. Remove the air duct.
2. Remove the No. 2 fan shroud.
3. Stretch the drive belt down and loosen the four nuts for the fan and clutch.

   Fig. 1: The fan blade is attached to the clutch with nuts, not all shown

4. Remove the nuts and the fan clutch with the cooling fan.

   Fig. 2: Once the nuts are removed, the blade comes off easily from the studs

   To install:

5. Install the fan clutch with the fan to the engine.
6. Install the fan nuts.
7. While retaining the drive belt, tighten the nuts to 10 ft. lbs. (13 Nm).
8. Install the No. 2 fan shroud.
9. Install the air duct.