#### REMOVAL & INSTALLATION

1. Remove the throttle body.
2. Remove the 4 screws to extract the IAC valve from the throttle body. Discard the gasket.

   Fig. 1: The IAC has a wiring harness attached to it

   To install:

3. Install a new gasket on the throttle body and place the IAC valve into position.
4. Secure the IAC valve on the throttle body.

   Fig. 2: Remove these four bolts to extract the IAC valve from the throttle body