#### REMOVAL & INSTALLATION

1. If the van is equipped with a C/D player, remove the amplifier to access the ABS ECM.
2. Remove the ABS ECM cover (if equipped) and the computer from the mounting bracket.
3. Disconnect the wiring from the ECM and remove the computer from the vehicle.

   To install:

4. Connect the harnesses and insert the wiring harness to the clamp.
5. Position the computer and install it with the 5 screws, tighten them to 48 inch lbs. (5 Nm).
6. Install the computer cover, if equipped.
7. Install the C/D amplifier if equipped.