#### 2TZ-FZE ENGINE

##### Engine and Automatic Transmission

The OBDII scan tool can clear DTC's, refer to the owners manual, or refer to the next few steps.

After repair of the circuit, the diagnostic code(s) must be removed from the ECM memory. With the ignition turned OFF, remove the 15 amp EFI fuse for 30 seconds or more. Once the time period has been observed, reinstall the fuse and check for normal code output.

If the diagnostic code is not erased, it will be retained by the ECM and appear along with a new code in event of future trouble.

Cancellation of the trouble code can also be accomplished by disconnecting the negative battery cable. However, disconnecting the battery cable will erase the other memory systems including the clock and radio settings. If this method is used, always reset these components once the trouble code has been erased.

Engine diagnostic codes — 2TZ-FE engine

Engine diagnostic codes — 2TZ-FE engine continued

Automatic transmission diagnostic codes — 2TZ-FE engine

Engine diagnostic codes — 2TZ-FZE engine

Engine diagnostic codes — 2TZ-FZE engine continued

Engine diagnostic codes — 2TZ-FZE engine continued

Engine diagnostic codes — 2TZ-FZE engine continued

Automatic transmission diagnostic codes — 2TZ-FZE engine