### Control Panel

#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable.
2. Remove the console box located below the ashtray.

   Fig. 1: Press on the sides of the box while pulling outwards to extract the console

3. Remove the ashtray retaining screws and disconnect the wiring.

   Fig. 2: Remove the four screws and retainer to extract the ash tray

4. Pull off the knobs prior to control panel removal.
5. Carefully pull out the center cluster finish panel.
6. Remove the control panel by removing the 4 screws.

   Fig. 3: Remove the four screws surrounding the control assembly and extract the unit from the dash

   To install:

7. Installation is the reverse of removal. Use care when snapping back together plastic components, if so equipped.