### Cold Start Injector

#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable.
2. Disconnect the cold start injector wiring.

   Fig. 1: Remove the wiring from the cold start injector

3. Place a suitable container or shop towel under the fuel pipe. Slowly remove the union bolt and two gaskets, the disconnect the fuel pipe.
4. Remove the two bolts and extract the cold start injector from the engine

   To install:

5. Place a new gasket on the cold start injector and secure to the engine with the bolts to 48 inch lbs. (5 Nm).
6. Using new gaskets, connect the fuel tube with the union bolts ands secure to 14 ft. lbs. (20 Nm). with gasket.
7. Connect the negative battery cable.
8. Start the engine and check for leaks.