### Slave Cylinder

#### REMOVAL & INSTALLATION

1. Raise and safely support the vehicle.
2. If equipped, remove the tension spring on the clutch fork.

   Fig. 1: Exploded view of the clutch slave (release) cylinder

3. Remove the hydraulic line from the release cylinder. Be careful not to damage the fitting.
4. Turn the release cylinder pushrod in sufficiently to gain clearance from the fork.
5. Remove the mounting bolts and withdraw the slave cylinder.
6. To install, reverse the removal procedures. Tighten the mounting bolts to 9 ft. lbs. (12 Nm). Tighten the hydraulic line to 11 ft. lbs. (15 Nm).
7. Bleed the clutch system. Adjust the fork tip clearance.