#### REMOVAL & INSTALLATION

The ignition coil is located under the passenger side floor near the distributor. Access is better from under the vehicle.

1. Turn the ignition key to the OFF position. Disconnect the negative battery cable.
2. Remove the exhaust pipe heat insulator if necessary.
3. Disconnect the high tension wire (running between the coil and the distributor) from the coil.

   Fig. 1: Release the clip on the tip of the coil wire

4. Disconnect the low tension wires from the coil.

   Fig. 2: Disconnect the low tension wiring from the coil

5. Loosen the coil bracket and remove the coil.

   Fig. 3: Remove these two mounting bolts

   Fig. 4: Extract the coil with bracket from the floor

   To install:

6. Install the new coil and secure the bracket.
7. Attach the low tension wires first, then the coil wire.
8. Install the exhaust heat insulator if removed.
9. Reconnect the negative battery cable.
10. Reset any various digital equipment such as radio memory and the clock if necessary.