### Control Cables

#### REMOVAL & INSTALLATION

1. Remove the control panel.
2. Disengage the adjusting clip at the heater/cooling unit end of the cable.
3. Disengage the end of the control cable from the control lever.
4. Remove the cable from the vehicle.

   To install:

5. Attach the cable to the end of the lever on the A/C or heater box.
6. Route the cable through the dash to the control lever and secure to the back of the unit.
7. Adjust the cable.
8. Install the control panel.