#### ALIGNMENT

Since the centering bolt, which has a chamfered shoulder, is used as the hood hinge and the lock set bolt, the hood and lock can't be adjusted with it on. To adjust properly, remove the hinge centering bolt and substitute a bolt with a washer for the centering bolt.

Fig. 1: Adjust the hood in the forward/rearward and left/right directions by loosening the bolts

To adjust the hood forward or rearward and left or right directions, adjust the hood by loosening the side hinge bolts and moving the hood to the desired position. Secure the hinge bolts.

To adjust the front edge of the hood in a vertical direction, turn the cushions as required.

Fig. 2: Turn the cushions on the hood for front edge adjustment

To adjust the hood lock, remove the 2 screws and the air inlet duct. Adjust the lock by loosening the lock retainer bolts. Tighten the hood lock mounting bolts and reinstall the air inlet duct when adjustment is complete.

Fig. 3: Loosen hood lock bolts, then position the lock bolts to adjust. Secure at the desired location