### Igniter

#### REMOVAL & INSTALLATION

1. Turn the ignition key to the OFF position. Disconnect the negative battery cable.
2. Separate the wiring harness connections.
3. Unbolt the igniter.
4. Loosen the nut holding the wire lead onto the coil.
5. Tag and disconnect the wire lead.
6. Lift the igniter off its mount.

   To install:

7. Mount the igniter to the bracket.
8. Attach the wire lead to the coil.
9. Connect the harness.
10. Connect the negative battery cable. Reset any digital equipment such as radio memory and the clock if necessary.