### Start Injector Time Switch

#### REMOVAL & INSTALLATION

1. Drain the engine coolant from the system.
2. Remove the right engine cover.
3. Locate the start injector time switch. The switch is located on the forward portion of the engine on the water outlet.
4. Remove the wiring from the switch.

   Fig. 1: Disconnect the wiring from the start injector time switch

5. Using a wrench, remove the switch from the outlet.

   To install:

6. Insert the switch into the threaded hole and secure.
7. Attach the wiring to the switch.
8. Fill the cooling system, start the engine and check for leaks.
9. Top off the system.
10. Install the right engine cover.