### Tailgate

#### REMOVAL & INSTALLATION

1. Open the tailgate completely.

   Fig. 1: Exploded view of the tailgate assembly

   Fig. 2: Exploded view of the tailgate internal components

2. Remove the inner trim panel.
3. Disengage the electrical connector from the combination light and the electric solenoid as required. Remove the harness and position out of the way.
4. Scribe the hinge location on the tailgate to aid in installation.
5. Disconnect the damper stay from the tailgate and position out of the way. Disconnect the rear defroster wiring, if equipped.
6. Remove the tailgate-to-hinge bolts and remove the tailgate from the vehicle.

   To install:

7. Position the tailgate on the vehicle and align the scribe marks.
8. Install the tailgate-to-hinge bolts and secure tightly.
9. Install the damper stay to the tailgate attaching the upper end to the tailgate first.
10. Reconnect the electrical harness as required.
11. Install the interior trim panel.
12. Close the tailgate slowly to check for proper alignment, and adjust as required.