#### OIL

The SAE (Society of Automotive Engineers) grade number indicates the viscosity of the engine oil; its resistance to flow at a given temperature. The lower the SAE grade number, the lighter the oil. For example, the mono-grade oils begin with SAE 5 weight, which is a thin light oil, and continue in viscosity up to SAE 80 or 90 weight, which are heavy gear lubricants. These oils are also known as "straight weight'', meaning they are of a single viscosity, and do not vary with engine temperature.

Multi-viscosity oils offer the important advantage of being adaptable to temperature extremes. These oils have designations such as 10W-40, 20W-50, etc. The "10W-40'' means that in winter (the "W'' in the designation) the oil acts like a thin 10 weight oil, allowing the engine to spin easily when cold and offering rapid lubrication. Once the engine has warmed up, however, the oil acts like a straight 40 weight, maintaining good lubrication and protection for the engine's internal components. A 20W-50 oil would therefore be slightly heavier than and not as ideal in cold weather as the 10W-40, but would offer better protection at higher rpm and temperatures because when warm it acts like a 50 weight oil. Whichever oil viscosity you choose when changing the oil, make sure you are anticipating the temperatures your engine will be operating in until the oil is changed again. Refer to the oil viscosity chart for oil recommendations according to temperature.

The API (American Petroleum Institute) designation indicates the classification of engine oil used under certain given operating conditions. Only oils designated for use "Service SH'' (or its superceding type) should be used. Oils of the SH type perform a variety of functions inside the engine in addition to the basic function as a lubricant. Through a balanced system of metallic detergents and polymeric dispersants, the oil prevents the formation of high and low temperature deposits and also keeps sludge and particles of dirt in suspension. Acids, particularly sulfuric acid, as well as other by-products of combustion, are neutralized. Both the SAE grade number and the APE designation can be found on top of the oil can.

Diesel engines also require SH engine oil. In addition, the oil must qualify for a CC rating. The API has a number of different diesel engine ratings, including CB, CC, and CD. Any of these other oils are fine as long as the designation CC appears on the can along with them. Do not use oil labeled only SH or only CC. Both designations must always appear together.

For recommended oil viscosity's, refer to the chart. Note that 10W-30 and 10W-40 grade oils are not recommended for sustained high speed driving when the temperature rises above the indicated limit.

##### Synthetic Oil

There are many excellent synthetic and fuel-efficient oils currently available that can provide better gas mileage, longer service life, and in some cases better engine protection. These benefits do not come without a few hitches, however, the main one being the price of synthetic oils, which is three or four times the price per quart of conventional oil.

Synthetic oil is not for every car and every type of driving, so you should consider your engine's condition and your type of driving. Also, check your car's warranty conditions regarding the use of synthetic oils.

Both brand new engines and older, high mileage engines are the wrong candidates for synthetic oil. The synthetic oils are so slippery that they can prevent the proper break-in of new engines; most manufacturer's recommend that you wait until the engine is properly broken in 5,000 miles (8,046km) before using synthetic oil.

Consider your type of driving. If most of your accumulated mileage is high speed, highway type driving, the more expensive synthetic oils may be of benefit. Extended highway driving gives the engine a chance to warm up, accumulating less acids in the oil and putting less stress on the engine over the long run. Under these conditions, the oil change interval can be extended (as long as your oil filter can last the extended life of the oil) up to the advertised mileage claims of the synthetics. Cars with synthetic oils may show increased fuel economy in highway driving, due to less internal friction. However, many automotive experts agree that 50,000 miles (80,465km) is too long to keep any oil in your engine.

Cars used under harder circumstances, such as stop-and-go, city type driving, short trips, or extended idling, should be serviced more frequently. For the engines in these cars, the much greater cost of synthetic or fuel-efficient oils may not be worth the investment. Internal wear increases much quicker on these cars, causing greater oil consumption and leakage.