### Air Cleaner (Element)

#### REMOVAL & INSTALLATION

1. Disconnect the Mass Air Flow (MAF) meter wiring.
2. Disconnect the A/C idle-up valve wiring.
3. Disconnect the 2 air hoses from the A/C idle-up valve.
4. Loosen the air cleaner hose clamp.

   Fig. 1: Unclasp the housing clips

5. Unclasp the 4 clips, and remove the air cleaner cap and MAF meter assembly.
6. Lift the air cleaner element out of the housing, clean and replace as necessary.

   Fig. 2: Lift the air cleaner lid and extract the filter from the housing

   Fig. 3: Inspect the air filter for dirt and damage

   To install:

7. Insert a new air cleaner element into the housing.
8. Place the air cleaner lid with MAF meter assembly into position and secure with the clips.
9. Attach all wiring to the air cleaner assembly.