#### CONTROL ARM BUSHING REPLACEMENT

1. Remove the lower control arm from the vehicle.
2. To remove the rear bushing, loosen the nut.
3. Force out the bushing and washer.

   To install:

4. Insert a bushing and position the washer as shown.

   Fig. 1: Place the washer into position and secure the bushing with the nut

5. Install the nut and tighten it so that the flat surface of the rear bushing is level with the upper surface of the lower control arm.
6. Tigthen the nut to 80 ft. lbs. (109 Nm).
7. Install the lower control arm.