#### CLEARING TROUBLE CODES

1. Turn the ignition switch to the ON position.
2. Disconnect the service connector, or pull the short pin, depending on the type your model has.
3. Using a jumper wire, connect terminals Tc and E1 of the DLC1
4. Depress the brake pedal 8 or more times within 3 seconds.
5. Chek that the warning light shows a normal code.
6. Attach the service connector or install the short pin.
7. Remove the jumper wire and double check the warning light is at normal code.

   ABS diagnostic codes — 2TZ-FE engine

   ABS diagnostic codes — 2TZ-FZE engine