### Coil Springs

#### REMOVAL & INSTALLATION

1. Raise and support the rear of the vehicle.
2. Remove the rear shock absorber.
3. Push down on the lower control arm enough to allow the coil spring to slide out.
4. Remove the upper and lower coil insulators. inspect and replace them if they are deteriorated.

   To install:

5. Install the coil spring on the lower control arm with the upper and lower insulators.
   1. Fit the lower end of the coil spring into the gap of the spring seat of the lower control arm.
6. Install the shock absorber.
7. Lower the vehicle.