#### LEVEL CHECK

NOTE: When the engine is cold, check the level of the supercharger dipstick. Inspect the supercharger oil every 30,000 miles (48,000 km).

1. Park the vehicle on a level spot and turn the engine off.
2. On the 4WD models, remove the left front suspension support member and the shift cable stay.
3. Turn the yellow headed supercharger oil level dipstick counterclockwise and pull it out.

   Fig. 1: The supercharger dipstick is yellow

4. Wipe the dipstick with a clean rag.
5. Reinsert the dipstick, turn it fully clockwise or the reading will not be correct.
6. Remove the dipstick again and look at the oil level on the end.
7. The oil level should be between the L and F marks on the dipstick.
8. If the level is low, check for leakage and Air Control Valve (ACV), and add oil up to the F mark.
9. Add supercharger oil through the dipstick tube using a vinyl tube and syringe. Recheck the oil level.

   Fig. 2: Using a syringe and vinyl tube, insert the supercharger oil into the dipstick tube

   NOTE: The supercharger could be damaged if it is overfilled or the oil level is low.

10. On the 4WD models, reinstall the left front suspension support member and shift cable assembly.