### Clutch Accumulator

#### REMOVAL & INSTALLATION

The clutch accumulator is located under the vehicle near the carbon canister.

Fig. 1: The clutch accumulator is located near the carbon canister

1. Raise and safely support the vehicle.
2. Remove the engine under cover.
3. Using a line wrench, disconnect the clutch liner leading to the accumulator.
4. Remove the two bolts holding the accumulator to the body and extract the unit.

   To install:

5. Postion the accumulator to the body of the vehicle and secure the bolts to 9 ft. lbs. (12 Nm).
6. Attach the line to the unit and secure the line union nut to 19 ft. lbs. (25 Nm).
7. Fill the clutch reservoir with brake fluid and bleed the system.
8. Check for leaks.
9. Install the engine under cover.