#### SEAL REPLACEMENT

There are two methods of replacing the oil seal depending on weather the oil pump cover is assembled to the engine or not.

If the oil pump is not installed to the timing chain case, use a flatbladed tool and rag to pry the old seal out. Apply multipurpose grease to the new oil seal lip. Using a seal installer, tap the seal into place.

Fig. 1: Place a rag over the retainer and carefully pry the seal out

Fig. 2: Install the seal using the proper sized driver

If the oil pump is installed on the timing chain case, use a knife to cut off the lip of the seal and pry it out. Check the oil seal lip contact surface of the crankshaft for cracks or damage. Apply multi-purpose grease to the new oil seal lip. Using a seal installer, drive the new seal flush against the cover edge.

Fig. 3: Carefully cut off the oil seal lip, then pry the seal from the cover

Fig. 4: Drive the seal flush against the cover edge