### Engine

One of the most common, if not THE most common, problems associated with trailer towing is engine overheating. If you have a cooling system without an expansion tank, you'll definitely need to get an aftermarket expansion tank kit, preferably one with at least a 2 quart capacity. These kits are easily installed on the radiator's overflow hose, and come with a pressure cap designed for expansion tanks.

Aftermarket engine oil coolers are helpful for prolonging engine oil life and reducing overall engine temperatures. Both of these factors increase engine life. While not absolutely necessary in towing Class I and some Class II trailers, they are recommended for heavier Class II and all Class III towing. Engine oil cooler systems usually consist of an adapter, screwed on in place of the oil filter, a remote filter mounting and a multi-tube, finned heat exchanger, which is mounted in front of the radiator or air conditioning condenser.