#### BREAKING IT IN

Make the first miles on the new engine, easy ones. Vary the speed but do not accelerate hard. Most importantly, do not lug the engine, and avoid sustained high speeds until at least 100 miles. Check the engine oil and coolant levels frequently. Expect the engine to use a little oil until the rings seat. Change the oil and filter at 500 miles, 1500 miles, then every 3000 miles past that.