#### ADJUSTMENTS

All models are equipped with self-adjusting rear drum brakes. Under normal conditions, adjustment of the rear brake shoes should not be necessary. However, if an initial adjustment is required insert the blade of a brake adjuster tool or a screw driver into the hole in the brake drum and turn the adjuster slowly. The tension is set correctly if the tire and wheel assembly will rotate approximately 3 times when spun with moderate force. Do not over adjust the brake shoes. Before adjusting the rear drum brake shoes, make sure emergency brake is in the OFF position, and all cables are free.