#### OPERATION IN FOREIGN COUNTRIES

If you plan to drive your car outside the United States or Canada, there is a possibility that fuels will be too low in anti-knock quality and could produce engine damage. It is wise to consult with local authorities upon arrival in a foreign country to determine the best fuels available.

### Engine

CAUTION
Prolonged and repeated skin contact with used engine oil, with no effort to remove the oil, may be harmful. Always follow these simple precautions when handling used motor oil:

- Avoid prolonged skin contact with used motor oil.
- Remove oil from skin by washing thoroughly with soap and water or waterless hand cleaner. Do not use gasoline, thinners or other solvents.
- Avoid prolonged skin contact with oil-soaked clothing.

The engine oil auto feeder system replaces the normal amount of oil consumed and does not lengthen the period of time between oil changes, so carry out the engine oil changes at the times prescribed.

If oil is poured only into the tank after the oil has been removed from the engine side, large quantities of oil are not immediately supplied to the engine, so always pour oil into the engine side.

The engine warning level light operates in response to the oil level sensor installed in the oil pan, so when the oil level warning light is lit up, it will not go off, even if oil is added to the oil tank.