#### REMOVAL & INSTALLATION

1. Remove the mounting screws and extract the sensor.

   Fig. 1: The throttle position sensor is located on the side of the throttle body

   To install:

2. Make certain the throttle plate is fully closed. With the throttle body held in its normal orientation, place the sensor onto the throttle body so that the electrical connector is in the correct position.
3. Turn the sensor clockwise as shown and temporarily install the retaining screws.
4. Adjust the throttle position sensor.