#### REMOVAL & INSTALLATION

1. Loosen the rear wheel lugnuts on the side of the vehicle you are performing work on.
2. Raise and support the rear of the vehicle. Remove the wheel.
3. Remove the rear caliper assembly.
4. Remove the rear brake disc.
5. Remove the parking brake shoes.
6. Using pliers, disconnect the parking brake cable form the parking brake shoe lever.

   Fig. 1: Use pliers to disconnect the parking brake cable from the lever . . .

   Fig. 2: . . . the lever has a hole to retain the cable

   To install:

7. Connect the parking brake cable to the parking brake shoe lever of the rear shoe.
8. Install the parking brake shoes.
9. Install the rear brake disc. Adjust the parking brake shoe clearance.
10. Install the rear caliper assembly.
11. Install the wheel, lower the vehicle and settle the parking brake shoes and disc.
12. Recheck and adjust the parking brake lever.