### Tail Lights

#### REMOVAL & INSTALLATION

1. Open the rear tailgate assembly.

   Fig. 1: Remove the two screws on the inside of the trunk area retaining the lamp

2. Remove the two retaining screws located on the inner portion of the lamp.
3. Pull the unit out towards the rear of the vehicle to extract the assembly.

   Fig. 2: Slide the tail light unit out towards the rear of the vehicle

   NOTE: There are two clips retaining the lamp in from the back, these may make removal tough.

4. Twist and remove the socket with bulbs attached from the back of the unit.

   Fig. 3: Twist and remove the socket from the back of the lamp

5. Twist and remove the bulbs as needed.

   Fig. 4: Twist and pull out the bulb from the socket

   To install:

6. Insert new bulb into the sockets.
7. Postion and secure the socket to the back of the assembly.
8. Place the lamp into position and pushing towards the front of the vehicle, secure the clamps.
9. Install and tighten the retaining screws.