### Seats

#### REMOVAL & INSTALLATION

The seat in the Previa van are all removed basically in the same manner. Some seats may have wiring near by that may need to be placed to the side to access the bolts.

Fig. 1: Pull this lever to lift up the drivers seat to access the engine compartment

Fig. 2: Removing the passengers side seat assembly

1. Locate the seat track retaining bolts. A cover may be hiding them.

   Fig. 3: View of the passengers side seat track rear retaining bolts

   Fig. 4: View of the passengers side seat track front retaining bolts

2. Remove the bolt covers.

   Fig. 5: Remove the covers on either side of the seat legs

3. Remove the seat track retaining bolts and extract the unit from the vehicle.

   To install:

4. Postion the seat with track onto the floorpan and secure with the retaining bolts.

   TORQUE SPECIFICATIONS

|