### Speakers

#### REMOVAL & INSTALLATION

##### Dash Mounted

1. Make sure that the radio is off.
2. Remove the speaker panel.
3. Remove the instrument panel box (some models).
4. Label and disconnect the speaker wires.
5. Remove the screws and extract the speaker.
6. Installation is the reverse of removal be sure to secure all components.

##### Door Mounted

1. Make sure that the radio is off.
2. On some models the armrest must be removed.
3. If equipped remove the power window switch or manual window handle.
4. Remove the upper door panel, then the lower door panel.
5. Label and disconnect the speaker wires.

   Fig. 1: Speaker bolt locations on most door mounted speakers

   Fig. 2: Label and disconnect the speaker wiring

6. Remove the 3 screws and the speaker.
7. Installation is the reverse of removal, secure all components.