#### HYDROCARBONS

Hydrocarbons (HC) are essentially fuel which was not burned during the combustion process or which has escaped into the atmosphere through fuel evaporation. The main sources of incomplete combustion are rich air/fuel mixtures, low engine temperatures and improper spark timing. The main sources of hydrocarbon emission through fuel evaporation on most vehicles used to be the vehicle's fuel tank and carburetor float bowl.

To reduce combustion hydrocarbon emission, engine modifications were made to minimize dead space and surface area in the combustion chamber. In addition, the air/fuel mixture was made more lean through the improved control which feedback carburetion and fuel injection offers and by the addition of external controls to aid in further combustion of the hydrocarbons outside the engine. Two such methods were the addition of air injection systems, to inject fresh air into the exhaust manifolds and the installation of catalytic converters, units that are able to burn traces of hydrocarbons without affecting the internal combustion process or fuel economy.

To control hydrocarbon emissions through fuel evaporation, modifications were made to the fuel tank to allow storage of the fuel vapors during periods of engine shut-down. Modifications were also made to the air intake system so that at specific times during engine operation, these vapors may be purged and burned by blending them with the air/fuel mixture.