#### ADJUSTMENT

1. Pull the parking brake lever all the way up and count the number of clicks. The correct number of clicks should be 4–5.
2. If necessary to adjust the parking brake, make sure that the rear brake shoe has been adjusted before making any adjustment at the parking brake handle.
3. Raise and safely support the vehicle. Loosen the two adjusting nuts and adjust parking brake cable No. 1 until travel is correct.